|  |  |
| --- | --- |
| **SOLID SURFACE QUOTE SHEET**PLASTIC LAMINATE COUNTERTOPS & FABRICATIONSPhone (610)-279-5230Fax (610)-279-3274Email or Fax this sheet to:quotes@generallaminate.com  | **Customer Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Phone: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Job Site Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** |
| **Edge Selection** | **Acrylic Color** | **Backsplash** | **Cutout** | **Sink Selection** |
| ❏ Euro Edge (Standard)❏ Bullnose Edge❏ Other: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \*\*All edge choices are standard 1-1/2” thickness unless specified otherwise. If thickness is different add in additional notes section.\*\* | Brand: **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**Color: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | ❏ Backsplash – 3” H (Vanity)❏ Backsplash – 4” H (Standard)❏ No backsplash❏ Other – Height: \_\_\_\_\_\_\_\_\_\_❏ Other – Coved (Commercial Use) | ❏ Sink Cutout❏ Cooktop Cutout❏ No Cutout❏ Other | ❏ Drop In Sink Supplied by Customer❏ Solid Surface Sink: *Circle Color.*BISQUE CAMEO WHITE BONE GLACIER WHITE❏ Stainless Steel Single Bowl Sink – Supplied by Fabricator❏ Stainless Steel Double Bowl Sink – Supplied by Fabricator❏ Sink supplied by others, mounted by Solid S. Fabricator. |
| **Range Information** | **Services** | **Additional Details** |
| ❏ Free Range ❏ Slide In Range | ❏ Template Only ❏ Delivery Only ❏ Template Copy (Provided by Customer) ❏ Template & Installation❏ Make to measurements, picked up & installed by others.  |  |

SKETCH BELOW, OR ATTACH SKETCH WITH THIS FORM. Mark Walls with “W”, Mark Finished Sides/Edges with “X”. Mark placement of appliances.